

--------------------- Network information ----------------------
Network summary:
 * Network appears to function ok.

Operating system:    Windows Xp or Later
Installed protocols: MSAFD-Tcpip [TCP/IP] (1001)
                     MSAFD-Tcpip [UDP/IP] (1002)
                     MSAFD-Tcpip [RAW/IP] (1003)
                     MSAFD-Tcpip [TCP/IPv6] (1004)
                     MSAFD-Tcpip [UDP/IPv6] (1005)
                     MSAFD-Tcpip [RAW/IPv6] (1006)
                     RSVP-TCPv6-Dienstanbieter (1007)
                     RSVP-TCP-Dienstanbieter (1008)
                     RSVP-UDPv6-Dienstanbieter (1009)
                     RSVP-UDP-Dienstanbieter (1010)
MSAFD-Tcpip [TCP/IP]MSAFD-Tcpip [UDP/IP]MSAFD-Tcpip [RAW/IP]MSAFD-Tcpip [TCP/IPv6]MSAFD-Tcpip [UDP/IPv6]MSAFD-Tcpip [RAW/IPv6]RSVP-TCPv6-DienstanbieterRSVP-TCP-DienstanbieterRSVP-UDPv6-DienstanbieterRSVP-UDP-Dienstanbieter
Adapter name:   Drahtlosnetzwerkverbindung
	Adapter index:  13
	Adapter id:     {CCCCFC86-2827-4EEE-B415-6FC8542BC152}
	Adapter Desc:   Hercules USB Wireless LAN Card
	Adapter medium: Native802_11
	Adapter Flags:  485
	Adapter MTU:    1500
	Adapter type:   Unknown
	Adapter IfType: IF_TYPE_IEEE80211
	Adapter Status: IfOperStatusUp
	Adapter Addr:   0-8-d3-8-22-b4 
	Adapter DNS:    192.168.2.1 	
MSAFD-Tcpip [TCP/IP]MSAFD-Tcpip [UDP/IP]MSAFD-Tcpip [RAW/IP]MSAFD-Tcpip [TCP/IPv6]MSAFD-Tcpip [UDP/IPv6]MSAFD-Tcpip [RAW/IPv6]RSVP-TCPv6-DienstanbieterRSVP-TCP-DienstanbieterRSVP-UDPv6-DienstanbieterRSVP-UDP-Dienstanbieter
Adapter name:   Drahtlosnetzwerkverbindung
	Adapter index:  13
	Adapter id:     {CCCCFC86-2827-4EEE-B415-6FC8542BC152}
	Adapter Desc:   Hercules USB Wireless LAN Card
	Adapter medium: Native802_11
	Adapter Flags:  485
	Adapter MTU:    1500
	Adapter type:   Unknown
	Adapter IfType: IF_TYPE_IEEE80211
	Adapter Status: IfOperStatusUp
	Adapter Addr:   0-8-d3-8-22-b4 
	Adapter DNS:    192.168.2.1 	
	IP Address:    192.168.2.117	mask: 255.255.255.0
MSAFD-Tcpip [TCP/IP]MSAFD-Tcpip [UDP/IP]MSAFD-Tcpip [RAW/IP]MSAFD-Tcpip [TCP/IPv6]MSAFD-Tcpip [UDP/IPv6]MSAFD-Tcpip [RAW/IPv6]RSVP-TCPv6-DienstanbieterRSVP-TCP-DienstanbieterRSVP-UDPv6-DienstanbieterRSVP-UDP-Dienstanbieter
Adapter name:   Drahtlosnetzwerkverbindung
	Adapter index:  13
	Adapter id:     {CCCCFC86-2827-4EEE-B415-6FC8542BC152}
	Adapter Desc:   Hercules USB Wireless LAN Card
	Adapter medium: Native802_11
	Adapter Flags:  485
	Adapter MTU:    1500
	Adapter type:   Unknown
	Adapter IfType: IF_TYPE_IEEE80211
	Adapter Status: IfOperStatusUp
	Adapter Addr:   0-8-d3-8-22-b4 
	Adapter DNS:    192.168.2.1 	
	IP Address:    192.168.2.117	mask: 255.255.255.0
	Gateway:        192.168.2.1
MSAFD-Tcpip [TCP/IP]MSAFD-Tcpip [UDP/IP]MSAFD-Tcpip [RAW/IP]MSAFD-Tcpip [TCP/IPv6]MSAFD-Tcpip [UDP/IPv6]MSAFD-Tcpip [RAW/IPv6]RSVP-TCPv6-DienstanbieterRSVP-TCP-DienstanbieterRSVP-UDPv6-DienstanbieterRSVP-UDP-Dienstanbieter
Adapter name:   Drahtlosnetzwerkverbindung
	Adapter index:  13
	Adapter id:     {CCCCFC86-2827-4EEE-B415-6FC8542BC152}
	Adapter Desc:   Hercules USB Wireless LAN Card
	Adapter medium: Native802_11
	Adapter Flags:  485
	Adapter MTU:    1500
	Adapter type:   Unknown
	Adapter IfType: IF_TYPE_IEEE80211
	Adapter Status: IfOperStatusUp
	Adapter Addr:   0-8-d3-8-22-b4 
	Adapter DNS:    192.168.2.1 	
	IP Address:    192.168.2.117	mask: 255.255.255.0
	Gateway:        192.168.2.1
	DHCP Enabled:   Yes
	DHCP Server:    192.168.2.1
	Lease Obtained: 192.168.2.1 1299572913
	Have Wins:      No
MSAFD-Tcpip [TCP/IP]MSAFD-Tcpip [UDP/IP]MSAFD-Tcpip [RAW/IP]MSAFD-Tcpip [TCP/IPv6]MSAFD-Tcpip [UDP/IPv6]MSAFD-Tcpip [RAW/IPv6]RSVP-TCPv6-DienstanbieterRSVP-TCP-DienstanbieterRSVP-UDPv6-DienstanbieterRSVP-UDP-Dienstanbieter
Adapter name:   Drahtlosnetzwerkverbindung
	Adapter index:  13
	Adapter id:     {CCCCFC86-2827-4EEE-B415-6FC8542BC152}
	Adapter Desc:   Hercules USB Wireless LAN Card
	Adapter medium: Native802_11
	Adapter Flags:  485
	Adapter MTU:    1500
	Adapter type:   Unknown
	Adapter IfType: IF_TYPE_IEEE80211
	Adapter Status: IfOperStatusUp
	Adapter Addr:   0-8-d3-8-22-b4 
	Adapter DNS:    192.168.2.1 	
	IP Address:    192.168.2.117	mask: 255.255.255.0
	Gateway:        192.168.2.1
	DHCP Enabled:   Yes
	DHCP Server:    192.168.2.1
	Lease Obtained: 192.168.2.1 1299572913

Adapter name:   LAN-Verbindung
	Adapter index:  12
	Adapter id:     {2878DDF3-B084-4801-A45D-8486879203D6}
	Adapter Desc:   Intel(R) 82566DC-2 Gigabit Network Connection
	Adapter medium: Unspecified
	Adapter Flags:  453
	Adapter MTU:    1500
	Adapter type:   MIB_IF_TYPE_ETHERNET
	Adapter IfType: IF_TYPE_ETHERNET_CSMACD
	Adapter Status: IfOperStatusDown
	Adapter Addr:   0-1d-9-17-c4-fa 
	Adapter DNS:    
MSAFD-Tcpip [TCP/IP]MSAFD-Tcpip [UDP/IP]MSAFD-Tcpip [RAW/IP]MSAFD-Tcpip [TCP/IPv6]MSAFD-Tcpip [UDP/IPv6]MSAFD-Tcpip [RAW/IPv6]RSVP-TCPv6-DienstanbieterRSVP-TCP-DienstanbieterRSVP-UDPv6-DienstanbieterRSVP-UDP-Dienstanbieter
Adapter name:   Drahtlosnetzwerkverbindung
	Adapter index:  13
	Adapter id:     {CCCCFC86-2827-4EEE-B415-6FC8542BC152}
	Adapter Desc:   Hercules USB Wireless LAN Card
	Adapter medium: Native802_11
	Adapter Flags:  485
	Adapter MTU:    1500
	Adapter type:   Unknown
	Adapter IfType: IF_TYPE_IEEE80211
	Adapter Status: IfOperStatusUp
	Adapter Addr:   0-8-d3-8-22-b4 
	Adapter DNS:    192.168.2.1 	
	IP Address:    192.168.2.117	mask: 255.255.255.0
	Gateway:        192.168.2.1
	DHCP Enabled:   Yes
	DHCP Server:    192.168.2.1
	Lease Obtained: 192.168.2.1 1299572913

Adapter name:   LAN-Verbindung
	Adapter index:  12
	Adapter id:     {2878DDF3-B084-4801-A45D-8486879203D6}
	Adapter Desc:   Intel(R) 82566DC-2 Gigabit Network Connection
	Adapter medium: Unspecified
	Adapter Flags:  453
	Adapter MTU:    1500
	Adapter type:   MIB_IF_TYPE_ETHERNET
	Adapter IfType: IF_TYPE_ETHERNET_CSMACD
	Adapter Status: IfOperStatusDown
	Adapter Addr:   0-1d-9-17-c4-fa 
	Adapter DNS:    
	IP Address:    0.0.0.0	mask: 0.0.0.0
MSAFD-Tcpip [TCP/IP]MSAFD-Tcpip [UDP/IP]MSAFD-Tcpip [RAW/IP]MSAFD-Tcpip [TCP/IPv6]MSAFD-Tcpip [UDP/IPv6]MSAFD-Tcpip [RAW/IPv6]RSVP-TCPv6-DienstanbieterRSVP-TCP-DienstanbieterRSVP-UDPv6-DienstanbieterRSVP-UDP-Dienstanbieter
Adapter name:   Drahtlosnetzwerkverbindung
	Adapter index:  13
	Adapter id:     {CCCCFC86-2827-4EEE-B415-6FC8542BC152}
	Adapter Desc:   Hercules USB Wireless LAN Card
	Adapter medium: Native802_11
	Adapter Flags:  485
	Adapter MTU:    1500
	Adapter type:   Unknown
	Adapter IfType: IF_TYPE_IEEE80211
	Adapter Status: IfOperStatusUp
	Adapter Addr:   0-8-d3-8-22-b4 
	Adapter DNS:    192.168.2.1 	
	IP Address:    192.168.2.117	mask: 255.255.255.0
	Gateway:        192.168.2.1
	DHCP Enabled:   Yes
	DHCP Server:    192.168.2.1
	Lease Obtained: 192.168.2.1 1299572913

Adapter name:   LAN-Verbindung
	Adapter index:  12
	Adapter id:     {2878DDF3-B084-4801-A45D-8486879203D6}
	Adapter Desc:   Intel(R) 82566DC-2 Gigabit Network Connection
	Adapter medium: Unspecified
	Adapter Flags:  453
	Adapter MTU:    1500
	Adapter type:   MIB_IF_TYPE_ETHERNET
	Adapter IfType: IF_TYPE_ETHERNET_CSMACD
	Adapter Status: IfOperStatusDown
	Adapter Addr:   0-1d-9-17-c4-fa 
	Adapter DNS:    
	IP Address:    0.0.0.0	mask: 0.0.0.0
	Gateway:        0.0.0.0
MSAFD-Tcpip [TCP/IP]MSAFD-Tcpip [UDP/IP]MSAFD-Tcpip [RAW/IP]MSAFD-Tcpip [TCP/IPv6]MSAFD-Tcpip [UDP/IPv6]MSAFD-Tcpip [RAW/IPv6]RSVP-TCPv6-DienstanbieterRSVP-TCP-DienstanbieterRSVP-UDPv6-DienstanbieterRSVP-UDP-Dienstanbieter
Adapter name:   Drahtlosnetzwerkverbindung
	Adapter index:  13
	Adapter id:     {CCCCFC86-2827-4EEE-B415-6FC8542BC152}
	Adapter Desc:   Hercules USB Wireless LAN Card
	Adapter medium: Native802_11
	Adapter Flags:  485
	Adapter MTU:    1500
	Adapter type:   Unknown
	Adapter IfType: IF_TYPE_IEEE80211
	Adapter Status: IfOperStatusUp
	Adapter Addr:   0-8-d3-8-22-b4 
	Adapter DNS:    192.168.2.1 	
	IP Address:    192.168.2.117	mask: 255.255.255.0
	Gateway:        192.168.2.1
	DHCP Enabled:   Yes
	DHCP Server:    192.168.2.1
	Lease Obtained: 192.168.2.1 1299572913

Adapter name:   LAN-Verbindung
	Adapter index:  12
	Adapter id:     {2878DDF3-B084-4801-A45D-8486879203D6}
	Adapter Desc:   Intel(R) 82566DC-2 Gigabit Network Connection
	Adapter medium: Unspecified
	Adapter Flags:  453
	Adapter MTU:    1500
	Adapter type:   MIB_IF_TYPE_ETHERNET
	Adapter IfType: IF_TYPE_ETHERNET_CSMACD
	Adapter Status: IfOperStatusDown
	Adapter Addr:   0-1d-9-17-c4-fa 
	Adapter DNS:    
	IP Address:    0.0.0.0	mask: 0.0.0.0
	Gateway:        0.0.0.0
	DHCP Enabled:   Yes
	DHCP Server:    
	Lease Obtained:  0
	Have Wins:      No

Routing table:
    Destination           Netmask           Nexthop  Interface    Metric                 Proto          Type        Age
---------------   ---------------   ---------------  ---------   -------   -------------------  ------------    -------
        0.0.0.0           0.0.0.0       192.168.2.1         13        25      PROTO_IP_NETMGMT  REMOTE_ROUTE      6471s
      127.0.0.0         255.0.0.0         127.0.0.1          1       306      PROTO_IP_NETMGMT   LOCAL_ROUTE      6548s
      127.0.0.1   255.255.255.255         127.0.0.1          1       306      PROTO_IP_NETMGMT   LOCAL_ROUTE      6548s
127.255.255.255   255.255.255.255         127.0.0.1          1       306      PROTO_IP_NETMGMT   LOCAL_ROUTE      6548s
    192.168.2.0     255.255.255.0     192.168.2.117         13       281      PROTO_IP_NETMGMT   LOCAL_ROUTE      6471s
  192.168.2.117   255.255.255.255     192.168.2.117         13       281      PROTO_IP_NETMGMT   LOCAL_ROUTE      6471s
  192.168.2.255   255.255.255.255     192.168.2.117         13       281      PROTO_IP_NETMGMT   LOCAL_ROUTE      6471s
      224.0.0.0         240.0.0.0         127.0.0.1          1       306      PROTO_IP_NETMGMT   LOCAL_ROUTE      6548s
      224.0.0.0         240.0.0.0     192.168.2.117         13       281      PROTO_IP_NETMGMT   LOCAL_ROUTE      6530s
255.255.255.255   255.255.255.255         127.0.0.1          1       306      PROTO_IP_NETMGMT   LOCAL_ROUTE      6548s
255.255.255.255   255.255.255.255     192.168.2.117         13       281      PROTO_IP_NETMGMT   LOCAL_ROUTE      6530s
